**ATRC-24，ATRC-36，ATRC-48**

* **The use of parts provided by other companies, our company has the right not to provide warranty service;**
* **Order replacement parts from authorized representatives and after-sale service agency.**
* **Provide the model number, serial number and description when you order components.**



|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **No.** | **Matters Code** | **Component name** | **Qty** | **Dimensions****(mm)/Model** | **Remark** |
| 1 | 301110001 | Adjustable steel legs | 4 | φ41.5\*100 | ATRC-24P\36P\48P |
| 2 | 21205001007 | Heat insulation tray assembly | 1 | 507\*620\*26.5 | ATRC-24P |
| 21205002007 | 807\*620\*26.5 | ATRC-36P |
| 21205003007 | 1117\*620\*26.5 | ATRC-48P |
| 3 | 301080002 | Galvanized flange nut | 6 | M6 | ATRC-24P |
| 9 | ATRC-36P |
| 11 | ATRC-48P |
| 4 | 301082001 | Galvanized flat washer | 4 | φ6\*φ10 | ATRC-24P |
| 6 | ATRC-36P |
| 7 | ATRC-48P |
| 5 | 21105001031 | Catch tray | 1 | 475\*187\*25 | ATRC-24P\36P\48P |
| 6 | 21105001008 | Control panel | 1 | 605\*185 | ATRC-24P |
| 21105002008 | 905\*185 | ATRC-36P |
| 21105003008 | 1215\*185 | ATRC-48P |
| 7 | 301030055 | Piezo Igniter | 2 | PE018A | ATRC-24P |
| 3 | ATRC-36P |
| 4 | ATRC-48P |
| 8 | 301140001 | Burner knob | 2 |  | ATRC-24P |
| 3 | ATRC-36P |
| 4 | ATRC-48P |
| 9 | 301081006 | Galvanized screw | 4 | ST4.8\*12.5 | ATRC-24P\36P\48P |
| 10 | 301080006 | A60 valve matching M16 nut | 4 |  | ATRC-24P |
| 6 | ATRC-36P |
| 8 | ATRC-48P |
| 11 | 301050012 | A60 valve matching Φ10 copper hoop | 6 |  | ATRC-24P |
| 9 | ATRC-36P |
| 12 | ATRC-48P |
| 12 | 301050009 | A60 valve matching air inlet joint | 2 |  | ATRC-24P |
| 3 |  | ATRC-36P |
| 4 |  | ATRC-48P |
| 13 | 301030012 | A60 valve with flame out protection device | 2 |  | ATRC-24P |
| 3 | ATRC-36P |
| 4 | ATRC-48P |
| 14 | 301040023（NAT）301040022（LP） | Nozzle (NAT)Φ2.4Nozzle (LP)Φ1.45 | 2 |  | ATRC-24P |
| 3 | ATRC-36P |
| 4 | ATRC-48P |
| 15 | 301080008 | M18 Copper lock nut | 2 |  | ATRC-24P |
| 3 | ATRC-36P |
| 4 | ATRC-48P |
| 16 | 301080007 | M16 Copper nut | 2 |  | ATRC-24P |
| 3 | ATRC-36P |
| 4 | ATRC-48P |
| 17 | 301050014 | Copper elbow | 234 |  | ATRC-24P |
| ATRC-36P |
| ATRC-48P |
| 18 | 21105001027 | Main fire gas pipe | 2 | Copper pipeΦ10 \*1.0 | ATRC-24P |
| 3 | ATRC-36P |
| 4 | ATRC-48P |
| 19 | 301060001 | 1/8”fitting | 1 | 1/8"-27NPT | ATRC-24P\36P\48P |
| 20 | 301060002 | Needle type pressure tap | 1 | M5\*23 | ATRC-24P\36P\48P |
| 21 | 301050013 | A60 valve matching 1/4 fire joint | 2 |  | ATRC-24P |
| 3 | ATRC-36P |
| 4 | ATRC-48P |
| 22 | 21105001026 | Pilot light intake-tube | 2 | Copper pipeΦ6\*0.8 | ATRC-24P |
| 3 | ATRC-36P |
| 4 | ATRC-48P |
| 23 | 301081002 | M4\*8 stainless steel recess head screw | 4 |  | ATRC-24P |
| 6 | ATRC-36P |
| 8 | ATRC-48P |
| 24 | 301030015 | Fire seat | 2 |  | ATRC-24P |
| 3 | ATRC-36P |
| 4 | ATRC-48P |
| 25 | 301030016 | Thermocouple | 2 | M9\*P1.0 L=600mm | ATRC-24P |
| 3 | ATRC-36P |
| 4 | ATRC-48P |
| 26 | 301170021 | Pilot light orifice | 2 |  | ATRC-24P |
| 3 | ATRC-36P |
| 4 | ATRC-48P |
| 27 | 301030029 | ignition needle | 2 |  | ATCB-24 |
| 3 |  | ATCB-36 |
| 4 |  | ATCB-48 |
| 28 | 21205001001 | Coutertop | 1 | 610\*700\*218 | ATRC-24P |
| 21205002001 | 910\*700\*218 | ATRC-36P |
| 21205003001 | 1220\*700\*218 | ATRC-48P |
| 29 | 301020006 | Grates | 4 | 150\*525\*22 | ATRC-24P |
| 6 | ATRC-36P |
| 8 | ATRC-48P |
| 30 | 21205001003 | Char grate back support brace | 1 | L=600 | ATRC-24P |
| 21205002003 | L=900 | ATRC-36P |
| 21205003003 | L=1210 | ATRC-48P |
| 31 | 301170002 | Short burner deflector | 2 | 92\*103 | ATRC-24P |
| 3 | ATRC-36P |
| 4 | ATRC-48P |
| 32 | 301170001 | Long burner deflector | 2 | L=451 | ATRC-24P |
| 3 | ATRC-36P |
| 4 | ATRC-48P |
| 33 | 301010007 | U-type burner | 2 |  | ATRC-24P |
| 3 | ATRC-36P |
| 4 | ATRC-48P |
| 34 | 301030023 | Pressure maintaining valve | 1 | RV48CLM-66-0012 CE | ATRC-24P\36P\48P |
| 35 | 301070020 | Gas manifold | 1 | Φ26-503\*648 | ATRC-24P |
| 301070021 | Gas manifold | Φ26-803\*648 | ATRC-36P |
| 301070022 | Gas manifold | Φ26-1113\*648 | ATRC-48P |
| 36 | 21205001005 | Surround | 1 | 610\*640\*203 | ATRC-24P |
| 21205002005 | 910\*640\*203 | ATRC-36P |
| 21205003005 | 1220\*640\*203 | ATRC-48P |

Model

|  |  |  |  |
| --- | --- | --- | --- |
| NameQty | ATRC-24P | ATRC-36P | ATRC-48P |
| Adjustable steel legs | 4 pieces（301110001） | 4 pieces（301110001） | 4 pieces（301110001） |
| Heat insulation tray | 1 piece（21205001007） | 1 piece（21205002007） | 1 piece（21205003007） |
| Catch tray | 1 piece（21105001031） | 1 piece | 1 piece |
| pressure maintaining valve | 1 piece（301030023） | 1 piece（301030023） | 1 piece（301030023） |
| Nozzle  | 2 piece（301040023） or（301040022） | 3 piece（301040023） or（301040022） | 4 piece（301040023） or（301040022） |
| No.7 Battery | 2 piece（306090005） | 3 piece（306090005） | 4 piece（306090005） |
| instructions | 1 piece（304080041） | 1 piece（304080041） | 1 piece（304080041） |