**ATMG-24，ATMG-36，ATMG-48**

* **The use of parts provided by other companies, our company has the right not to provide warranty service;**
* **Order replacement parts from authorized representatives and after-sale service agency.**
* **Provide the model number, serial number and description when you order components.**



|  |  |  |  |
| --- | --- | --- | --- |
| **No.** | **Matters Code** | **Component name** | **Dimensions(mm)/Model** |
| 1 | 21102001021 | Catch tray | 490\*196\*25 |
| 2 | 301080002 | M6 nut |  |
|
|
| 3 | 301082001 | Φ6\*Φ10 galvanized flat |  |
|
|
| 4 | 21202001006 | Control panel | 605\*185 |
| 21202002006 | 905\*185 |
| 21202003006 | 1215\*185 |
| 5 | 301030055 | Piezo Igniter | PE018A |
|
|
| 6 | 301140001 | Control knob |  |
|
|
| 7 | 301081006 | Galvanized screw | ST4.8\*12.5 |
| 8 | 301060001 | 1/8”fitting | 1/8"-27NPT |
| 9 | 301060002 | Needle type pressure tap | M5\*23 |
| 10 | 301080006 | A60 valve matching M16 nut |  |
|
|
| 11 | 301050012 | A60 valve matching Φ10 copper hoop |  |
|
|
| 12 | 301050009 | A60 valve matching air inlet joint |  |
|
|
| 13 | 301030012 | A60 valve with flame out protection device |  |
|  |
|  |
| 14 | 301040023（NAT）301040022（LP） | Nozzle (NAT) Φ2.4Nozzle (LP) Φ1.45 |  |
|
|
| 15 | 301080008 | M18 Copper lock nut |  |
|
|
| 16 | 301080007 | M16 Copper nut |  |
|
|
| 17 | 301050014 | Copper elbow |  |
|
|
| 18 | 21105001027 | Main fire gas pipe | Copper pipe Φ10 \*1.0 |
|
|
| 19 | 301050013 | A60 valve matching 1/4 fire joint |  |
|
|
| 20 | 21105001026 | Pilot light intake-tube | Copper pipe Φ6\*0.8 |
|
|
| 21 | 301081002 | M4\*8 stainless steel recess head screw |  |
|
|
| 22 | 301030016 | Thermocouple  | M9\*P1.0 L=600mm |
|
|
| 23 | 301030015 | Fire seat |  |
|
|
| 24 | 301170021 | Pilot light orifice |  |
|
|
| 25 | 301030029 | ignition needle |  |
|
|
| 26 | 21202001001 | Countertop | 610\*700\*218 |
| 21202002001 | 910\*700\*218 |
| 21202003001 | 1220\*700\*218 |
| 27 | 301010007 | U-type burner |  |
|
|
| 28 | 301030023 | Pressure maintaining valve | RV48CLM-66-0012 CE |
| 29 | 301070023 | Intake-tube（flame out protection device） | Φ26-503\*648 |
| 301070024 | Φ26-803\*648 |
| 301070025 | Φ26-1113\*648 |
| 30 | 21202001004 | Bottom border package | 610\*670\*257 |
| 21202002004 | 910\*670\*257 |
| 21202003004 | 1220\*670\*257 |
| 31 | 301110001 | Adjustable steel legs | φ41.5\*100 |
|
|

|  |  |  |  |
| --- | --- | --- | --- |
| QtyModelName | ATMG-24P | ATMG-36P | ATMG-48P |
| Adjustable steel legs | 4 pieces（301110001） | 4 pieces（301110001） | 4 pieces（301110001） |
| Catch tray | 1 piece（21102001021） | 1 piece（21102001021） | 1 piece（21102001021） |
| pressure maintaining valve | 1 piece（301030023） | 1 piece（301030023） | 1 piece（301030023） |
| Nozzle  | 2 piece（301040023） or（301040022） | 3 piece（301040023） or（301040022） | 4 piece（301040023） or（301040022） |
| No.7 Battery | 2 piece（306090005） | 3 piece（306090005） | 4 piece（306090005） |
| instructions | 1 piece（304080043） | 1 piece（304080043） | 1 piece（304080043） |

Model