**AT7G4BO-1**

**Explosive view of product and parts**

* **The use of parts provided by other companies, our company has the right not to provide warranty service;**
* **Order replacement parts from authorized representatives and after-sale service agency.**
* **Provide the model number, serial number and description when you order components.**







|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **No.** | **Matters Code** | **Component name** | **Qty** | **Dimensions (mm)/Model** | **Notes** |
| 1 | 301020022 | Cooking grates | 2 | 580\*380 |  |
| 2 | 301060097 | Slide rail frame fixed column | 2 | φ16\*7 |  |
| 3 | 301060060 | Slider rack pin | 4 | φ8\*26 |  |
| 4 | 301080047 | Stainless steel hexagonal nut | 4 | M6 |  |
| 5 | 21103020037 | Slider rack | 2 |  |  |
| 6 | 301140001 | Knob | 5 |  |  |
| 7 | 301030055 | Piezo Igniter | 1 | PE018A |  |
| 8 | 21203020007 | Oven door assembly | 1 |  |  |
| 9 | 21103020047 | Underside face plate of oven | 1 |  |  |
| 10 | 21203011005 | Control panel | 1 |  |  |
| 13 | 301030080 | temperature limiter | 1 |  |  |
| 14 | 21103020044 | Fire hole cover | 1 |  |  |
| 15 | 21303020043 | Stove base plate | 1 |  |  |
| 16 | 301100030 | Stove net rack | 1 | 650\*530 |  |
| 17 | 301110010 | Gravity foot | 4 | φ51\*（102-152） |  |
| 18 | 21303020045 | Radiant panel of stove | 1 |  |  |
| 23 | 301020039 | Burner body | 2 | 7kw |  |
| 301030085 | 301030085 | Pilot Assemblies (hot plate) | 2 | B880205B-1STD | long |
| 25 | 301081063 | Stainless steel hexagonal screw | 4 | M5\*12 |  |
| 26 | 301050012 | Copper hoop | 5 | Φ10 |  |
| 27 | 301080007 | Copper nut | 5 | M16 |  |
| 28 | 301050098 | Male copper elbow | 4 | M14 to 1-8 PT |  |
| 29 | 301050099 | Copper nut | 4 | M14 |  |
| 31 | 21103020046 | Ejector tube base | 4 |  |  |
| 32 | 301081064 | Zinc plated hexagonal screw | 8 | M5\*8 |  |
| 35 | 301020036 | Burner lid | 2 | 7kw |  |
| 36 | 301020026 | Ejector tube | 2 | 7kw |  |
| 37 | 301040063 | Hot plates burner nozzle(7kw) | 2 | 202 (20mbar) |  |
| 301040072 | 210 (25mbar) |
| 301040074 | 2 | 130 (30mbar) |  |
| 301040073 | 125 (37mbar) |
| 301040064 | 120 (50mbar) |
| 38 | 301020030 | Air regulation tube(Hot plate) | 2 | 7kw |  |
| 39 | 301020035 | Burner lid | 2 | 3.5kw |  |
| 40 | 301020038 | Burner body | 2 | 3.5kw |  |
| 41 | 301020025 | Ejector tube | 2 | 3.5kw |  |
| 42 | 301020029 | Air regulation tube(Hot plate) | 2 | 3.5kw |  |
| 43 | 301040061 | Hot plates burner nozzle(3.5kw) | 2 | 140 (20mbar) |  |
| 301040069 | 145 (25mbar) |  |
| 301040071 | 2 | 092 (30mbar) |  |
| 301040070 | 085 (37mbar) |  |
| 301040062 | 080 (50mbar) |  |
| 44 | 21203020014 | Pilot Assemblies (hot plate) | 2 | B880205B-1STD | short |
| 45 | 301050096 | input pipe | 1 |  |  |
| 46 | 301060099 | Copper hoop | 5 | φ4 |  |
| 47 | 301060098 | Joint | 5 | M10\*1.0-φ4 |  |
| 49 | 301050023 | copper hoop | 10 | φ10 |  |
| 50 | 301080006 | A60 valve matching nut | 10 | M16 |  |
| 52 | 301030016 | Thermocouple（back/ hot plate） | 2 | T101625 L=600 |  |
| 53 | 301030012 | A60 valve | 4 |  |  |
| 54 | 301050009 | A60 valve matching air inlet joint | 5 |  |  |
| 57 | 301030090 | Thermocouple（front/ hot plate） | 2 | T101625 L=300 |  |
| 59 | 301060001 | pressure measuring connector | 1 | NPT 1/8"-27 |  |
| 60 | 301060002 | pressure measuring connector screw | 1 | M5\*23 |  |
| 63 | 301050045 | Main fire intake pipe of oven | 1 | Bellows φ10 |  |
| 64 | 301050025 | Copper joint | 1 | M16 to1-8 PT |  |
| 65 | 301080008 | Bronze locknut | 1 |  |  |
| 66 | 301040067 | Oven burner nozzle(8kw) | 1 | 210 (20mbar) |  |
| 301040078 | 220 (25mbar) |  |
| 301040080 | 1 | 140 (30mbar) |  |
| 301040079 | 130 (37mbar) |  |
| 301040068 | 125 (50mbar) |  |
| 68 | 301010024 | Stove burner | 1 |  |  |
| 69 | 21103020050 | Temperature sensor stator | 1 |  |  |
| 70 | 305010070 | Connect wires (Piezo Igniter ) | 1 | L=1200mm |  |
| 71 | 21103020038 | Pilot Assemblies stator | 1 |  |  |
| 72 | 301030084 | Pilot Assemblies (Oven) | 1 |  |  |
| 73 | 21103020063 | Pilot fire intake pipe of oven | 1 | Copper pipeφ4 |  |
| 74 | 301030078 | Thermocouple（oven） | 1 | T101625 L=1500 |  |
| 75 | 305010072 | Connect wires (temperature limiter) | 2 | L=500mm |  |
| 76 | 301030077 | A65T valve | 1 |  |  |
| 80 | 21103020061 | Pilot fire intake pipe of hot plate | 2 | Copper pipeφ4 | back |
| 81 | 21103020057 | Main fire intake pipe of hot plate | 1 | Copper pipeφ10 | back |
| 82 | 21103020059 | Main fire intake pipe of hot plate | 1 | Copper pipeφ10 | front |
| 83 | 21103020062 | Pilot fire intake pipe of hot plate | 2 | Copper pipeφ4 | front |
| 85 | 21103020060 | Main fire intake pipe of hot plate | 1 | Copper pipeφ10 | front |
| 87 | 21103020058 | Main fire intake pipe of hot plate | 1 | Copper pipeφ10 | back |
| 89 | 301090011 | Remove drip tray | 2 |  |  |

**Accessories List**

|  |  |  |  |
| --- | --- | --- | --- |
| name | code | | quantity |
| Gravity foot | 301110005 | | 4 pieces |
| Nozzle(7kw)  Hot Plate | 301040063 | 202 (20mbar) | 2 piece |
| 301040072 | 210 (25mbar) |
| 301040074 | 130 (30mbar) |
| 301040073 | 125 (37mbar) |
| 301040064 | 120 (50mbar) |
| Nozzle(3.5kw)  Hot Plate | 301040061 | 140 (20mbar) | 2 piece |
| 301040069 | 145 (25mbar) |
| 301040071 | 092 (30mbar) |
| 301040070 | 085 (37mbar) |
| 301040062 | 080 (50mbar) |
| Nozzle(8kw)  Oven | 301040067 | 210 (20mbar) | 1 piece |
| 301040078 | 220 (25mbar) |
| 301040080 | 140 (30mbar) |
| 301040079 | 130(37mbar) |
| 301040068 | 125 (50mbar) |
| S.S Stand | 21103012040 | | 1 piece |
| Instructions | 304080403 | | 1 piece |

Our products have the advantages of good durability and low maintenance charge. But to update some components and necessary maintenance, can prolong life length of the products. Contact the dealer for assistance. To avoid confusion, please follow the format of “Explosive view of product and parts” in this manual.