**ATFS-40，ATFS-50，ATFS-75**

* **The use of parts provided by other companies, our company has the right not to provide warranty service;**
* **Order replacement parts from authorized representatives and after-sale service agency.**
* **Provide the model no., serial no. and description when you order components.** 

|  |  |  |  |
| --- | --- | --- | --- |
| **No.** | **Matters Code** | **Component name** | **Dimensions****(mm)/Model** |
| 1 | 21201001001 | Body assembly | 394\*746\*751 |
| 21201003001 | 534\*746\*751 |
| 1.1 | 21101001039 | Oil drain pipe fixer |  |
| 2 | 301060017 | Lower Hinge assembly |  |
| 3 | 21201001007 | Door assemble assembly | 392\*34\*529 |
| 21201003007 | 532\*34\*529 |
| 4 | 301060016 | Upper Hinge assembly |  |
| 5 | 21101001032 | Front panel |  |
| 21101003032 |  |
| 6 | 301050011 | Oil drain valve |  |
| 7 | 301030027(NG) 301030028(LP) | Pilot burner-NG pilot burner-LP | Z95369Z95370 |
| 301030050 | Thermocouple | 21628 |
| 7.1 | 301030031 | ignition needle |  |
| 8 | 301010009 | burner | Y-0006 |
|
|
| 9 | 301100003 | Flat screen | 342\*342\*φ8 |
| 301100004 | 482\*342\*φ8 |
| 10 | 301100001 |  Fry basket | 337\*165\*178 |
| 301100002 | 337\*235\*178 |
| 11 | 21101001036 | Hanging plate | 392\*161\*1.2 |
| 21101003034 | 532\*161\*1.2 |
| 12 | 21201001005 | External upper smokestack assemble assembly | 396\*240\*158 |
| 21201003005 | 536\*240\*158 |
| 13 | 21201001006 | Internal upper smokestack assemble assembly | 278\*268\*98 |
| 21201002006 | 348\*268\*98 |
| 21201003006 | 418\*268\*98 |
| 14 | 21201001009 | Fry tank assembly | 397\*706\*438 |
| 21201002009 | 397\*706\*438 |
| 21201003009 | 537\*706\*438 |
| 15 | 301060011 | Orifice fitting |  |
|
|
| 16 | 301040021 (NG)301040025 (LP) | Orifice (NG)Orifice (LP) |  NG240(NG) NG135(LP) |
|
|
| 17 | 301050006 | Pilot gas line | bellows\φ6.35\*580 |
| 18 | 301170012 | Intake-tube combination valve |  |
| 19 | 301070010 | Strap-intake-tube | 3/4 |
| 20 | 301050008 | Reducing elbow | 3/4 |
| 21 | 301050010 | Pipe coupling | 3/4 |
| 22 | 301030026 (NG)301030025 (LP) | Combination safety valve | 4K7721498 (NG)4K77224A4 (LP) |
| 23 | 301050007 | Pipe union | 3/4 |
| 24 | 301070016 | Gas manifold assembly |  |
| 301070017 |  |
| 301070018 |  |
| 25 | 301030005 | Temperature limiter | LCCM200300000 |
| 26 | 301030024 | thermostat | RX-17-30 199℃/390F |
| 27 | 21101001038 | Temperature control mounting plate |  |
| 27.1 | 301030030 | Electronic pulse ignition | QD 1.5-1 |
| 28 | 301140006 | Temperature control knob |  |
| 29 | 301110002 | Adjustable steel |  |
| 30 | 301060001 | Needle type pressure tap |  |
| 31 | 301060002 | Needle type pressure tap |  |

|  |  |  |  |
| --- | --- | --- | --- |
| QtyName | ATFS-40P | ATFS-50P | ATFS-75P |
| Adjustable steel leg | 4 pieces（301110002） | 4 pieces（301110002） | 4 pieces（301110002） |
| Frying basket | 2 piece（301100001） | 2 piece（301100001） | 2 piece（301100002） |
| Flat screen | 1 piece（301100003） | 1 piece（301100003） | 1 piece（301100004） |
| Oil drain pipe | 1 piece（301060006） | 1 piece（301060006） | 1 piece（301060006） |
| External upper smokestack assembly | 1 piece（21201001005） | 1 piece（21201001005） | 1 piece（21201003005） |
| Internal upper smokestack assembly | 1 piece（21201001006） | 1 piece（21201002006） | 1 piece（21201003006） |
| U.S. six angle flange head tapping screws | 4pieces（301081006） | 4pieces（301081006） | 4pieces（301081006） |
| U.S. six angle tapping screws | 2pieces（301081009） | 2pieces（301081009） | 2pieces（301081009） |
| Hanging plate | 1 piece（21101001036） | 1 piece（21101001036） | 1 piece（21101003034） |
| No.7 Battery | 1 piece（306090005） | 1 piece（306090005） | 1 piece（306090005） |
| Instructions | 1 piece（304080044） | 1 piece（304080044） | 1 piece（304080044） |